Carpet Finishes (Fitted with gripper)
Acoustilay perimeter strips are nailed or glued around the
perimeter of the room with the black barrier layer facing down
and the acoustic seal, compressed by two thirds, to the wall or
skirting board. Carpet gripper rods are then nailed in place on
top of the perimeter strip, raising them to the correct height to
take the carpet. Acoustilay panels are tightly butted up to the
perimeter detail, and loose laid in brick bond pattern onto the
existing floorboards or Maxiboard panels.

If you are unsure of which product or system you require, please
contact our industry leading technical department on Tel: 01204
380074 or email info@soundreduction.co.uk for free, friendly
advice.

	

		

Sound Reduction Systems Ltd
Adam St, Off Lever St, Bolton BL3 2AP
Tel: +44 (0)1204 380074 · Fax: +44 (0)1204 380957
E-mail: info@soundreduction.co.uk
Web: www.soundreduction.co.uk       

SRS Ltd Acoustic Insulation Datasheets
Sound Reduction Systems Ltd are experts in all areas of sound
insulation. For further information on their range of products and
systems for reducing sound transmission in buildings and meeting
the acoustic requirements of the Building Regulations Approved
Document E, please see the following datasheets, which are easily
obtained by calling 01204 380074 or downloading from
www.soundreduction.co.uk.
Ceilings:
• Maxi 60 Ceiling
• Maxiboard beneath existing plasterboard / lath and plaster
• Maxiboard beneath concrete beam and block
• Maxiboard on a British Gypsum MF ceiling
Walls:
• Maxi HP Partition System
• Maxiboard installed with new/existing stud
• Maxiboard installed on new/existing masonry
Floors:
• Maxideck
• SubPrimo
If you are unsure of which product or system you require, please
contact our industry leading technical department on Tel: 01204
380074 or email info@soundreduction.co.uk for free, friendly
advice.