h  MODEM DEFINITION
h
p[1] Modem Name:
c40

h
h********************************************
h  RESULT CODE DEFINITIONS
h********************************************
h
p[2] Acknowledge:
c 40

p[3] Connect 300 baud:
c 40

p[4] Ring detected:
c 40

p[5] No carrier:
c 40

p[6] Error:
c 40

p[7] Connect 1200 baud:
c 40

p[8] Connect 2400 baud:
c 40

p[9] Connect 4800 baud:
c 40

p[10] Connect 9600 baud:
c 40

p[12] Connect 14400 baud:
c 40

p[11] Response from Go Local command:
c 40

u[13]
u[14]
u[15]
u[16]
u[17]
u[18]
u[19]
u[20]
u[21]
u[22]
u[23]
u[24]
u[25]
u[26]
u[27]
u[28]
u[29]
u[30]
u[31]
h
p[32] Result Code Wait (.01 sec.):
n 0,999
200
h
h********************************************
h  MODEM WAKEUP(initialization) SEQUENCES
h********************************************
h
h
p[33] Wakeup #1:
c 40

p[34] Result:
c 40

p[35] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[36] Wakeup  #2:
c 40

p[37] Result:
c 40

p[38] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[39] Wakeup  #3:
c 40

p[40] Result:
c 40

p[41] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[42] Wakeup  #4:
c 40

p[43] Result:
c 40

p[44] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[45] Wakeup  #5:
c 40

p[46] Result:
c 40

p[47] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[48] Wakeup  #6:
c 40

p[49] Result:
c 40

p[50] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[51] Wakeup  #7:
c 40

p[52] Result:
c 40

p[53] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[54] Wakeup  #8:
c 40

p[55] Result:
c 40

p[56] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[57] Wakeup  #9:
c 40

p[58] Result:
c 40

p[59] Wait (.01 sec.):
n 0,999
0
h
h********************************************
h  MODEM COMMAND DEFINITIONS
h********************************************
h
p[60] Before dial:
c 40

p[61] Result:
c 40

p[62] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[63] Answer phone:
c 40

p[64] Result:
c 40

p[65] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[66] Abort answer:
c 40

p[67] Result:
c 40

p[68] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[69] Before answer:
c 40

p[70] Result:
c 40

p[71] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[72] GOTO carrier(originate mode):
c 40

p[73] Result:
c 40

p[74] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[75] GOTO carrier(answer mode):
c 40

p[76] Result:
c 40

p[77] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[78] GOTO voice:
c 40

p[79] Result:
c 40

p[80] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[81] Hangup(modem control method):
c 40

p[82] Result:
c 40

p[83] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[84] Set wait for Carrier:
c 40

p[85] Result:
c 40

p[86] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[87] Go local from Answer mode:
c 40

p[88] Result:
c 40

p[89] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[90] Go local from Originate mode:
c 40

p[91] Result:
c 40

p[92] Wait (.01 sec.):
n 0,999
0
u
u____________________________________________
u
u (Will not override settings)
u[93] Dial phone:
u 40
u
u[94] Result:
u 40
u
u[95] Wait (.01 sec.):
u 0,999
u
h
h____________________________________________
h
p[96] Before Go Local from Originate mode:
c 40

p[97] Result:
c 40

p[98] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[99] Before Go Local from Answer mode:
c 40

p[100] Result:
c 40

p[101] Wait (.01 sec.):
n 0,999
0
h
h____________________________________________
h
p[102] Legal Dial String Characters:
c 40

u[103]
u[104]
u[105]
u[106]
u[107]
u[108]
u[109]
u[110]
u[111]
u[112]
u[113]
u[114]
u[115]
u[116]
u[117]
u[118]
u[119]
u[120]
u[121]
u[122]
u[123]
u[124]
u[125]
u[126]
u[127]
u[128]
h
h
h********************************************
h COMMUNICATIONS MODEM CONTROL PARAMETERS
h********************************************
h
h Issue Wakeup (initialization) sequence:
h
m[129] after hangup:
1
Yes No
m[130] before dial:
1
Yes No
m[131] before answer:
1
Yes No
h____________________________________________
h
h Hangup command via hardware or modem control:
h
m[132] Hangup via removal of DTR(hardware method):
1
Yes No
h____________________________________________
h
h Sync Port to Connect Baud Rate:
h
m[133]  After Answer Connection:
1
Yes No
m[134]  After Dial   Connection:
2
Yes No
h____________________________________________
h
h Initialize Modem Using Current Baud rate:
h   (no implies initialization at 300 baud)
h
m[135]
2
Yes No
h____________________________________________
h
h  Allow Modem to Auto-answer phone:
h
m[136]
2
Yes No
u[137]
u[138]
u[139]
u[140]
u[141]
u[142]
u[143]
u[144]
$
